# Taken from here

[Create a 6dof IMU with a gyro and accelerometer for (Arduino) multicopters. (brokking.net)](http://www.brokking.net/imu.html)

Great explanation here


<https://lastminuteengineers.com/mpu6050-accel-gyro-arduino-tutorial/>

# Axis Explained

Diagram

Description automatically generatedA blue circuit board with green arrows

Description automatically generated



# Basics

Gyroscope sensitivity

Angular velocity LSB/(degree/second) Note, 16bit

+/- 250 d/s 131

+/- 500 d/s 65.5

+/- 1000 d/s 32.8

+/- 2000 d/s 16.4

## Example to get degrees from degrees/second

So if Zaxis constantly rotating for +/-500 d/s, at 6d/s we get 393

Then angleDegreesPerSecond = rawGyro/65.5

Take this 393 and multiply by 60

393x60 = 23580

So 23580/65.5 = 360 ie in 1 minute the gyro will rotate 360d (6d/second)

If we sample this at say 250Hz (0.25ms), and add to previous value we can end up with degrees/angle

250Hz = 0.25ms

By ZaxisRaw / 250 / 65.5


= ZaxisRaw \* 0.0000611

So

Angle\_pitch += rawGyroX \* 0.0000611;

Angle\_roll += rawGyroY \* 0.0000611;

Problem with the above



To fix this we can combine both axis:

Gy -= Gx \* sin(RawGyroZ \* 0.0000166 \* (3.142 / 180) > need to convert to radians

Gx += Gy \* sin(RawGyroZ \* 0.0000166 \* (3.142 / 180)